# EC Function Description:

1. Realize bypass power supply function

# Instructions for using EC by flashing with a U disk:

1. Prepare a FAT32 formatted U disk.

2. Download the EC file compression package, extract it, and place the files in the root directory of the U disk.



3. There are risks in flashing the device, be sure to connect it to a power source during operation, otherwise it may cause the handheld device to fail to start up.

4. Shut down and then turn on the device, press F7 to enter the boot menu, select booting from the FAT32 disk, and the script will run automatically. Occasionally there may be a black screen restart, just retry it.s